Current BITA Guidance Notes
GN 9	90° Stacking aisle widths	
GN15	Fork lift truck leaf chains maintenance and inspection	
GN19	Engine rating specifications for use in literature	
GN26	Testing steering kick-back for 4 wheeled industrial counterbalanced trucks	
GN28	Thorough examination & safety inspections of industrial lift trucks	
GN29	Truck control levers	
GN40	Handling of single suspended loads by rider controlled counterbalanced & reach trucks	
GN43	Integral attachments for industrial lift trucks	
GN44	Rough terrain high lift telescopic handlers training guidance	
GN45	Double deep stacking and stability tests and rating	
GN49	Engineers working at heights	
GN50	Tyre tread wear	
GN51	Specification for indicator lights for container handling and piggy-back operations	
GN52	Industrial trucks – floor surfaces and gradients	
GN53	Double deep stacking operations	
GN54	Specification for longitudinal load moment indicators for variable reach trucks	
GN55	Compliance with the machinery directive and application of the CE Mark	
GN56	Drive-In and drive-through racking	
GN57	Industrial trucks on public roads	
GN60	Operator restraint + HSE information sheet ‘Fitting & use of restraining systems on lift trucks.’	
GN61	Planning & Management of Construction Sites for the Safe Use of Rough Terrain Telescopic Handlers	
GN62	Maintenance, inspection & repair of fork arms & attachments	
GN63	Solid Tyre Fitting Guidance	
GN64	Press Fitting of Solid Tyres	
GN65	Overhead Guard (Fops) Damage